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        嘟嘟车-三排 Tuk Tuk
产品技术参数表Product Technical Specifications
	                    序号Serialnumber
	项目名称
Project name
	参数paramneter
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	技术参数 technical parameters
	整车尺寸
Overall dimensions
	3435X1375X1850mm
	

	
	额定乘员
Rated capacity
	7人 /7people
	

	
	轴距
Wheelbase
	2720mm
	

	
	轮距
track width
	1200mm
	

	
	最小离地间隙
Ground clearance
	205mm
	

	
	最小转弯半径
Minimum Turning Radius
	4.5m
	

	
	最大运行速度
Maximum operating speed
	60km/h
	

	
	最大爬坡度
Maximum Gradability
	25%
	

	
	整备质量
curb weight
	450kg（不含电池）
Excluding battery
	

	
	额定载荷
curb weight
	500kg
	

	
	续驶里程
range
	150km
	

	
	充电时间
Chargeing time
	8小时
8Hours
	

	电气系统electrical system
	电机
motor
	72V4500W交流异步电机
60/72V4500W AC asynchronous motor

	
	控制器
Controller
	72V4500W交流异步控制器
60/72V4500W AC asynchronous motor

	
	电池
Battery
	72V150AH磷酸铁锂电池
72V150AH Lithium Iron Phosphate Battery

	
	充电器
charger
	车载式智能全自动充电器
Vehicle-mounted intelligent fully automatic charger

	
	灯光及信号
Light and Signal
	LED大灯、左右转向灯、刹车灯、行车灯、仪表、电喇叭、倒车喇叭。
LED Headlights, Left and Right Turn Signals, Brake Lights, Running Lights,Instrument (Panel), Electric Horn, Reverse Horn

	底盘系统electrical system
	车架
frame
	整体焊接车架+酸洗磷化电泳烤漆
Integral Welded Frame + Acid Pickling, Phosphating, Electrophoretic Coatingand Baking Paint

	
	动力传动
power transmission
	后置驱动,配备前进和倒档
Rear-Mounted Drive, Equipped with Forward and Reverse Gears

	
	转向
Steering System
	龙头把式转向机构
Handlebar-Type Steering Mechanism

	
	悬架
Suspension
	前悬架：加粗双摇臂弹簧式前叉
Front Suspension：Double wishbone spring fork

	
	后悬挂
Rear suspension
	汽车级球笼式独立减震传动系统
Automotive-Grade Constant Velocity (CV) Joint-Type Independent ShockAbsorption Transmission System

	
	制动
Braking

	前后三轮鼓式液压制动 + 脚踏机械驻车制动
Front and Rear Three-Wheel Drum-Type Hydraulic Brakes + Foot-OperatedMechanical Parking Brake

	
	轮胎
tyre
	前轮：125/65—12 后轮：125/65—12
Front Wheel：125/65—12 Rear Wheel：125/65—12

	车身配置Body configuration
	油漆
Paint
	高级汽车专用油漆
High-Grade Automotive-Specific Paint

	
	车体
Vehidle Body
	钢制车架+一体冲压成型车体
Steel Frame + Integrally Stamped Vehicle Body 

	
	仪表台
IP
	注塑成型仪表台，电门锁，仪表，组合开关
Injection-Molded Instrument Panel, Electric Door Lock, Instrument (Gauge),Combination Switch

	
	座椅
Seat
	注塑底板发泡海绵皮革软座椅+靠背
Soft Seat with Injection-Molded Base, Foam Sponge and Leather + Backrest


规格和细节如有变动恕不另行通知。
Specifications and details are subject to change without notice。

性能特点	

· 车架主梁采用40X80MM，3MM厚方管，采用独立悬挂后桥，骑行舒适重安全。
· 灯光及信号：前大灯、前后转向灯、侧转向灯、组合后尾灯均为LED，并设有电喇叭和倒车蜂鸣器。 The main beam of the frame is made of 40X80MM square tubes with a thickness of 3MM, and is equipped withan independent suspension rear axle,ensuring comfortable riding and emphasizing safety.
·   Lights and signals: The front headlights, front and rear turn signals, side turn signals, and combined rear taillightsare all LED, and are equipped with an electric horn and a reverse buzzer
· 


[image: 微信图片_20251229160449_503_87][image: 微信图片_20251229160424_502_87][image: 微信图片_20251229160309_501_87][image: 微信图片_20251229160129_500_87][image: 微信图片_20251229160109_499_87][image: 微信图片_20251229160019_498_87][image: 微信图片_20251229160615_505_87]     [image: 微信图片_20251229160531_504_87]

image5.jpeg




image6.jpeg




image7.jpeg




image8.jpeg




image9.jpeg




image1.png




image2.jpeg




image3.jpeg




image4.jpeg




